1. Unzip and copy all files into the root directory of a USB thumbdrive

2. Plug the USB thumbdrive into the NMT

3. Browse to the USB device and use the File Icon to browse to usbupdate.html

4. Press Enter on usbupdate.html, and another Enter on the listed firmware update link.

5. Firmware update will commence and will automatically reboots after done.

6. After NMT boots up with new firmware, if a NMT applications update is
   needed, the NMT applications update Wizard will start automatically.

7. Follow through the steps and select to update from USB.

8. NMT applications update will commence and will automatically reboots after it is done.

9. Firmware and NMT applications update is completed at this point